**Tender specification text**

**Wall sleeves**

***Fiber cement***

**Wall sleeve made of asbestos-free fiber cement for the installation of annular seals**

Wall sleeve with smooth internal wall and closed circular grooves on the external wall

to be delivered and – according to the indications on the drawing – installed flush within the shuttering during the structuring work (before pouring the concrete) and secured against dislocation.

Product:

DDL Wall Sleeve fiber cement

DDL GmbH, 73249 Wernau / N.

or equivalent

Inside diameter of the wall sleeve: DN/ID ….…..…...… mm

Installation length of the wall sleeve: L ….….…....… mm

Material: Asbestos-free fiber cement

Model/Name: Fiber cement DN…….…..…

Amount of wall sleeves: Pcs. ………..…………..

 Unit price: ……………€ Total price: ………………..€

